Scaling Upas

Erik Quanstrom

quanstro@coraid.com

ABSTRACT

The Plan 9 email system, Upas, uses traditional methods of delivery to

UNIX ® mail boxes while using a user-level file system, Upas/fs, to trans-

late mail boxes of various formats into a single, convenient format for

access. Unfortunately, it does not do so efficiently. Upas/fs reads entire

folders into core. When deleting email from mail boxes, the entire mail

box is rewritten. I describe how Upas/fs has been adapted to use cach-

ing, indexing and a new mail box format (mdir) to limit I/O, reduce core

size and eliminate the need to rewrite mail boxes.

1. Introduction

Chained at his root two scion demons dwell

� Erasmus Darwin, The Botanic Garden

At Coraid, email is the largest resource user in the system by orders of magnitude. As

of July, 2007, rewriting mail boxes was using 300MB/day on the WORM and several

users required more than 400MB of core. As of July, 2008, rewriting mail boxes was

using 800MB/day on the WORM and several users required more than 1.2GB of core to

read email. Clearly these are difficult to sustain levels of growth, even without growth

of the company. We needed to limit the amount of disk space used and, more urgently,

reduce Upas/fs � core size.

The techniques employed are simple. Mail is now stored in a directory with one mes-

sage per file. This eliminates the need to rewrite mail boxes. Upas/fs now maintains an

index which allows it to present complete message summaries without reading indexed

messages. Combining the two techniques allows Upas/fs to read only new or refer-

enced messages. Finally, caching limits both the total number of in-core messages and

their total size.

2. Mdir Format

In addition to meeting our urgent operational requirements of reducing memory and

disk footprint, to meet the expectations of our users we require a solution that is able to

handle folders up to ten thousand messages, open folders quickly, list the contents of

folders quickly and support the current set of mail readers.

There are several potential styles of mail boxes. The maildir[1] format has some attrac-

tive properties. Mail can be delivered to or deleted from a mail box without locking.

New mail or deleted mail may be detected with a directory scan. When used with WORM

storage, the amount of storage required is no more than the size of new mail received.

Mbox format can require that a new copy of the inbox be stored every day. Even with

storage that coalesces duplicate blocks such as Venti, deleting a message will generally

require new storage since messages are not disk-block aligned. Maildir does not reduce

the cost of the common task of a summary listing of mail such as generated by acme

Mail.

The mails[2] format proposes a directory per mail. A copy of the mail as delivered is

stored and each mime part is decoded in such a way that a mail reader could display the

file directly. Command line tools in the style of MH[3] are used to display and process

mail. Upas/fs is not necessary for reading local mail. Mails has the potential to reduce

memory footprint below that offered by mdirs for native email reading. However all of

the largest mail boxes at our site are served exclusively through IMAP. The preformat-

ting by mails would be unnecessary for such accounts.

Other mail servers such as Lotus Notes[4] store email in a custom database format

which allows for fielded and full-text searching of mail folders. Such a format provides

very quick mail listings and good search capabilities. Such a solution would not lend

itself well to a tool-based environment, nor would it be simple.

Maildir format seemed the best basic format but its particulars are tied to the UNIX envi-

ronment; mdir is a descendant. A mdir folder is a directory with the name of the folder.

Messages in the mdir folder are stored in a file named utime.seq . Utime is defined as

the decimal UNIX seconds when the message was added to the folder. For the inbox,

this time will correspond to the UNIX � From � line. Seq is a two-digit sequence number

starting with 00. The lowest available sequence number is used to store the message.

Thus, the first email possible would be named 0.00. To prevent accidents, message

files are stored with the append-only and exclusive-access bits turned on. The mes-

sage is stored in the same format it would be in mbox format; each message is a valid

mbox folder with a single message.

3. Indexing

When upas/fs finds an unindexed message, it is added to the index. The index is a file

named foldername .idx and consists a signature and one line per MIME part. Each line

contains the SHA1 checksum of the message (or a place holder for subparts), one field

per entry in the messageid/info file, flags and the number of subparts. The flags are

currently a superset of the standard IMAP flags. They provide the similar functionality to

maildir � s modified file names. Thus the � S � (answered) flag remains set between invoca-

tions of mail readers. Other mutable information about a message may be stored in a

similar way.

Since the info file is read by all the mail readers to produce mail listings, mail boxes may

be listed without opening any mail files when no new mail has arrived. Similarly, open-

ing a new mail box requires reading the index and checking new mail. Index files are

typically between 0.5% and 5% the size of the full mail box. Each time the index is gen-

erated, it is fully rewritten.

4. Caching

Upas/fs stores each message in a Message structure. To enable caching, this struc-

ture was split into four parts: The Idx (or index), message subparts, information on the

cache state of the message and a set of pointers into the processed header and body.

Only the pointers to the processed header and body are subject to caching. The avail-

able cache states are Cidx , Cheader and Cbody .

When the header and body are not present, the average message with subparts takes

roughly 3KB of memory. Thus a 10,000 message mail box would require roughly 30MB

of core in addition to any cached messages. Reads of the info or subject files can

be satisfied from the information in the Idx structure.

Since there are a fair number of very large messages, requests that can be satisfied by

reading the message headers do not result in the full message being read. Reads of the

header or rawheader files of top-level messages are satisfied in this way. Reading

the same files for subparts, however, results in the entire message being read. Caching

the header results in the Cheader cache state.

Similarly, reading the body requires the body to be read, processed and results in the

Cbody cache state. Reading from MIME subparts also results in the Cbody cache

state.

The cache has a simple LRU replacement policy. Each time a cached member of a mes-

sage is accessed, it is moved to the head of the list. The cache contains a maximum

number of messages and a maximum size. While the maximum number of messages

may not be exceeded, the maximum cache size may be exceeded if the sum of all the

currently referenced messages is greater than the size of the cache. In this case all

unreferenced messages will be freed. When removing a message from the cache all of

the cacheable information is freed.

5. Collateral damage

Each new user of a new system uncovers a new class of bugs.

� Brian Kernighan

In addition to upas/fs, programs that have assumptions about how mail boxes are struc-

tured needed to be modified. Programs which deliver mail to mail boxes (deliver, mar-

shal, ml, smtp) and append messages to folders were given a common (nedmail) func-

tion to call. Since this was done by modifying functions in the Upas common library,

this presented a problem for programs not traditionally part of Upas such as acme Mail

and imap4d. Rather than fold these programs into Upas, a new program, mbappend,

was added to Upas.

Imap4d also requires the ability to rename and remove folders. While an external pro-

gram would work for this as well, that approach has some drawbacks. Most importantly,

IMAP folders can � t be moved or renamed in the same way without reimplementing func-

tionality that is already in upas/fs. It also emphasises the asymmetry between reading

and deleting email and other folder actions. Folder renaming and removal were added

to upas/fs. It is intended that mbappend will be removed soon and replaced with equiv-

alent upas/fs functionality � at least for non-delivery programs.

Mdirs also expose an oddity about file permissions. An append-only file that is mode

0622 may be appended to by anyone, but is readable only by the owner. With a direc-

tory, such a setup is not directly possible as write permission to a directory implies per-

mission to remove. There are a number of solutions to this problem. Delivery could be

made asymmetrical � incoming files could be written to a mbox. Or, following the exam-

ple of the outbound mail queue, each user could deliver to a directory owned by that

user. In many BSD-derived UNIX systems, the � sticky bit � on directories is used to mod-

ify the meaning of the w bit for users matching only the other bits. For them, the w bit

gives permission to create but not to remove.

While this is somewhat of a one-off situation, I chose to implement a version of the

� sticky bit � using the existing append-only bit on our file server. This was implemented

as an extra permission check when removing files. Fewer than 10 lines of code were

required.

6. Performance

A representative local mail box was used to generate some rough performance num-

bers. The mail box is 110MB and contains 868 messages. These figures are shown in

table 1. In the worse case � an unindexed mail box � the new upas/fs uses 18% of the

memory of the original while using 13% more cpu. In the best case, it uses only 5% of

the memory while using only 13% of the cpu. Clearly, a larger mail box will make these

ratios more attractive. In the two months since the snapshot was taken, that same mail

box has grown to 220MB and contains 1814 messages.

______________________________________________________

Table 1 � Performance ______________________________________________________

action user system real core size

s s s MB ______________________________________________________

old fs read 1.69 0.84 6.07 135 ______________________________________________________

initial read 1.65 0.90 6.90 25 ______________________________________________________

indexed read 0.64 0.03 0.77 6.5 ______________________________________________________ ç ç ç ç ç ç ç ç

ç ç ç ç ç ç ç

ç ç ç ç ç ç ç

ç ç ç ç ç ç ç

ç ç ç ç ç ç ç

ç ç ç ç ç ç ç ç

7. Future Work

While Upas � memory usage has been drastically reduced, it is still a work-in-progress.

Caching and indexing are adequate but primitive. Upas/fs is still inconsistently

bypassed for appending messages to mail boxes. There are also some features which

remain incomplete. Finally, the small increase in scale brings some new questions

about the organization of email.

It may be useful for mail boxes with very large numbers of messages to divide the index

into fixed-size chunks. Then messages could be read into a fixed-sized pool of struc-

tures as needed. However it is currently hard to see how clients could easily interface a

mail box large enough for this technique to be useful. Currently, all clients assume that

it is reasonable to allocate an in-core data structure for each message in a mail box. To

take advantage of a chunked index, clients (or the server) would need a way of limiting

the number of messages considered at a time. Also, for such large mail boxes, it would

be important to separate the incoming messages from older messages to limit the work

required to scan for new messages.

Caching is particularly unsatisfactory. Files should be read in fixed-sized buffers so

maximum memory usage does not depend on the size of the largest file in the mail box.

Unfortunately, current data structures do not readily support this. In practice, this limi-

tation has not yet been noticeable.

There are also a few features that need to be completed. Tracking of references has

been added to marshal and upas/fs. In addition, the index provides a place to store

mutable information about a message. These capabilities should be built upon to pro-

vide general threading and tagging capabilities.

8. Speculation

Freed from the limitation that all messages in a mail box must be read and stored in

memory before a single message may be accessed, it is interesting to speculate on a few

further possibilites.

For example, it may be useful to replace separate mail boxes with a single collection of

messages assigned to one or more virtual mail boxes. The association between a mes-

sage and a mail box would be a � tag. � A message could be added to or removed from

one or more mail boxes without modifying the mdir file. If threads were implemented

by tagging each message with its references, it would be possible to follow threads

across mail boxes, even to messages removed from all mail boxes, provided the under-

lying file were not also removed. If a facility for adding arbitrary, automatic tags were

enabled, it would be possible to tag messages with the email address in the SMTP From

line.

9. References

[1]D. Bernstein, � Using maildir format � , published online at

http://cr.yp.to/proto/maildir.html

[2]F. Ballesteros published online at http://lsub.org/magic/man2html/1/mails

[3]MH Wikipedia entry, http://en.wikipedia.org/wiki/MH_Message_Handling_System

[4]Lotus Notes Wikipedia entry, http://en.wikipedia.org/wiki/Lotus_Notes

[5]D. Presotto, � Upas � a Simpler Approach to Network Mail � , Proceedings of the 10th

Usenix conference, 1985.